WinAVR on Win98

\_delay\_ms() causes Internal compiler error

It is a matter of the CPU.

A Pentium MMX cant do a CMOVLE Instruction.

Its for AMD K6-2 and above.

# Ref

<https://sourceforge.net/p/winavr/mailman/winavr-users/?viewmonth=200810>